====================================================================================================
== Release Note (tdlSConvE) ========================================================================

[] V19.070 : 2019/07/05

  + First release of Program in English and English Documentation.



[] V19.100 : 2019/10/25

  + Solved the problem that the conversion may stop abnormally when program ends or conversion
    operation is stopped due to inadequate license specification.

  + LSH (Local String Header) of Multi Byte Text String item can be output to communication trace
    file by specifying (TRCTTYPE&0x4000) of .ini.



[] V20.040 : 2020/04/17

  + With the revision accompanying the update of TDS, connection and disconnection performance of
    HSMS-SS and HSMS-GS was improved.

  + Solved the problem that connection/disconnection of new connection was reported for existing
    connection when there was a new connection when existing connection was prioritized during 
    Passive operation in HSHS connection, and existing connection was also disconnected.



[] V21.060 : 2021/06/15

  + [ViewLastLine] has been newly added to menu to facilitate positioning to last line of trace
    display. 



[] V21.060b :2023/07/05

  + Both 32bit AP and 64-bit AP are available.

  + Each sample file is stored in Sample0/.
    After installation and before the first boot, it is recommended that you copy .ini file that
    exists in Sample0/ to the directory (Win32/ or Win64/) where the .exe exists, if necessary.



[] V24.040 : 2024/04/15

  + During HSMS communication, messages can be sent and received by setting the most significant
    bit of SystemByte in the communication message header to =1 (that is, if SystemByte is treated
    as a 32-bit signed integer, it will be a negative value).

