====================================================================================================
== Release Note (tdlSSim) ==========================================================================

[] V19.070 : 2019/07/05

  + First release of Program in English and English Documentation.



[] V19.100 : 2019/10/25

  + LSH (Local String Header) can be specified in Multi Byte Text String item in SML format message
    definition file.
    Specify 'M99' (99:LSH value) as the mnemonic when specifying Multi Byte Text String (022).

  + DEVID=0 can be specified for script execution.

  + Revised to display section name used at start of simulation when section name is not specified.

  + Solved the problem that display of message definition file to be used remains as an input value
    if it ends abnormally at simulation start.

  + Solved the problem that the sequence display section was not positioned at the beginning of the
    program line indicating the selected sequence when the program was started.

  + Solves the problem that the simulation may stop abnormally when simulation is stopped due to
    incomplete simulation or when simulation is terminated.

  + Corresponding to the change of magnified display on Windows (Control Panel -- 100, 125, 150%
    specified on display).
    This solved the disorder of the variable display pane.



] V20.040 : 2020/04/17

  + With the revision accompanying the update of TDS, connection and disconnection performance of
    HSMS-SS and HSMS-GS was improved.

  + Solved the problem that connection/disconnection of new connection was reported for existing
    connection when there was a new connection when existing connection was prioritized during 
    Passive operation in HSHS connection, and existing connection was also disconnected.

  + The following revisions have been made to the processing device selection combo box.
    - Solved the problem that selected device was reselected due to Select and Deselect request
      processing from connection destination when connecting to HSMS-GS.
    - Solved the problem that display of '*' was not updated even if Select status of selected
      device changed when HSMS-GS was connected.

